****

****

****

**ThermaStar by Pella 10 Series Left-Operable Vinyl Double Pane Annealed New Construction Egress Sliding Window (Rough Opening: 48-in x 60-in; Actual: 47.5-in x 59.5-in)**

Share

[**email**](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series#noop)

Only at Lowe's

**ThermaStar by Pella 10 Series Left-Operable Vinyl Double Pane Annealed New Construction Egress Sliding Window (Rough Opening: 48-in x 60-in; Actual: 47.5-in x 59.5-in)**

Item #: 329312 |  Model #: 748171614571



****

Be the first to **write a review!**

**Share this product:**

****

**$194.85**





* **[Description](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series" \l "description-tab)**

* **[Specifications](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series" \l "specifications-tab)**

* **[Protection Plans](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series" \l "warranties_tab)**

* **[Reviews](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series" \l "reviews_tab)**

* **[Community Q&A](http://www.lowes.com/pd_329312-1257-748171614571___?productId=3193165&pl=1&Ntt=therma+star+by+pella+10+series" \l "prodAnswerTab)**

**Description**

**Got an update or addition to this product's details? Share it here.**

10 Series Left-Operable Vinyl Double Pane Annealed New Construction Egress Sliding Window (Rough Opening: 48-in x 60-in; Actual: 47.5-in x 59.5-in)

* Advanced Low-E energy-saving glass
* Argon gas is inserted between the 2 panes of glass for added energy efficiency
* Maintenance-free vinyl frames
* Sliding sash can be removed to clean exterior glass from inside your home
* Interlocking sashes on windows helps seal out drafts and improve energy efficiency
* Custom sizes and color-matched grilles are also available via special order
* For more product details refer to the specifications tab

**Specifications**

**Got an update or addition to this product's details? Share it here.**

|  |  |
| --- | --- |
| Actual Height (Inches) | 59.5 |
| Actual Width (Inches) | 47.5 |
| Rough Opening Width (Inches) | 48 |
| Rough Opening Height (Inches) | 60 |
| Jamb Depth (Inches) | 1.63 |
| Series | 10 |
| Interior Color/Finish | White |
| Exterior Color/Finish | White |
| Hardware Color/Finish | White |
| Paintable | No |
| Color/Finish Family | White |
| Frame Material | Vinyl |
| Includes Grid | No |
| Grid Type | N/A |
| Grid Width | N/A |
| Grid Profile | N/A |
| Grid Pattern | N/A |
| Glazing Type | Double pane |
| Argon Gas Insulated | Yes |
| Glass Strength | Annealed |
| Obscure Glass | No |
| Frame Profile | Flat |
| Screen Included | Half |
| Screen Type | Fiberglass mesh |
| Screen Frame Type | Roll-form |
| Roller Type | Vinyl rollers |
| Sash Operation (Exterior View) | Left-operable |
| Sash Configuration | 2-lite |
| Warranty | Limited lifetime |
| Lowe's Exclusive | Yes |
| Project Type | New construction |
| Meets Egress Requirement | Yes |
| Lock Type | Cam |
| Nail Fin | Integrated |
| J Channel | N/A |
| Mulling | N/A |
| Wood Jamb Extension | None |
| Number of Locks | 1 |
| Ventilation Latches | N/A |
| Impact Glass | No |
| Hurricane Approved | No |
| Sound Transmission Control (STC) Rated | Yes |
| Design Pressure (DP) Rating | 30 |
| U Value | 0.3 |
| Solar Heat Gain Coefficient (SHGC) | 0.3 |
| ENERGY STAR Qualified Northern Zone | Yes |
| ENERGY STAR Qualified North/Central Zone | Yes |
| ENERGY STAR Qualified South/Central Zone | Yes |
| ENERGY STAR Qualified Southern Zone |  |