SUBSURFACE INSPECTION PROCEDURES

**Please call 874-8703 or 874-8693(ONLY)**

**Or email** **buildinginspections@portlandmaine.gov**

With the issuance of this permit, the owner, applicant, installer or their designee is required to provide adequate notice to the City of Portland Inspection Services for the following inspections. Appointments must be requested at least 24 hours in advance of the required inspection. The inspection date will need to be confirmed by this office.

* Please read any conditions of approval that are attached to this permit!! Contact this office if you have any questions.
* **Permit expires unless work is commenced within 24 months of the date of issuance**
* **If the inspection requirements are not followed as stated below additional fees may be incurred due to the issuance of a “Stop Work Order” and subsequent release to continue with construction.**

 **120 Brackett Ave. Peaks Island**

**CBL: 087I I004**

**City Permit # 2013-02031**

**State ID# 12072**

**Septic Field**

1. After Site Preparation: Septic field and extension inspection for bottom preparation/ scarification to verify removal of vegetation and roughened surface, established transitional horizon and erosion and sedimentation control measures.
2. Prior to covering the system: Inspection of system components including stone, pipes or proprietary devices, tanks, hay, filter fabric, and fill beneath and beside the disposal area before backfill. Also included are curtain drains, diversion ditches, berms or other measures outlined in the design.

**The project cannot move to the next phase prior to the required inspection and approval to continue, REGARDLESS OF THE NOTICE OR CIRCUMSTANCES.**