36 W.Commonwealth rd, Portland, Maine, 04103 
CBL # 298 D007 001

Specification:    Additional information

Flooring

The finished flooring -  VCT tile

Gutter/Downspout - No 

Foundation     There is no current foundation

Proposed foundation : ( appendix A )  

12" diam. x 6 " high concrete footing below frost line ( more than 48" deep) 
8" diam. x 46"  high concrete pier
Anchor bolt 
Metal post base
PT 4"x 4" post

 The Door

Spec on the actual door:   EMCO  36 in. x 80 in. 100 Series White Self-Storing Storm Door - 

https://www.homedepot.com/p/EMCO-36-in-x-80-in-100-Series-White-Self-Storing-Storm-Door-E1SS-36WH/100081634  

The mudroom is not heated.

The Roof

The roof is flashed with Aluminum Flashing - 6" on the wall, 6" on the roof. Flashing on the wall is counter flashed with Grace Ice & Water Membrane - 12" high ( Appendix B)

The existing vent, cables etc.

The location of the existing vent, cables and wires will not be changed.
Flood light will be placed on the exterior wall of the mudroom.