Viessman vitoden 100 Wall mounted under the laundry room in the basement with Polly propylene venting through the sidewall.

Baseboard mounted her heat loss app -10° outdoors to maintain 70° indoor

Boiler is mounted to plywood screwed to the wall