126 Sherwood

REQUEST FOR MORE INFORMATION

06/11/17

1. There is no plan for steps to have backers.
2. For top of bottom stringers to landing:

Drawing A

Tie: <https://www.strongtie.com/deckconnectors_decks/lsc_connect/p/lsc>

For bottom of top stringers to landing:

Drawing B

Tie: <https://www.strongtie.com/facemounthangersssl_solidsawnlumberconnector/luc-lu-u-hu-huc_productgroup_wcc/p/luc.lu.u.hu.huc>

1. Drawing A

Tie: <https://www.strongtie.com/deckconnectors_decks/lsc_connect/p/lsc>

1. Drawing C

Tie: <https://www.strongtie.com/deckties_decks/dtt_tie/p/dtt>

Tie: <https://www.strongtie.com/facemounthangersssl_solidsawnlumberconnector/luc-lu-u-hu-huc_productgroup_wcc/p/luc.lu.u.hu.huc>

1. Drawing D

Handrail material:

<http://www.homedepot.com/catalog/pdfImages/c1/c11359f3-f978-40bc-9d32-2389cb3d316c.pdf>

1. Post base with 1/2” threaded rod, nut and washer: <https://www.strongtie.com/retrofitpostbases_postbases/aba-abu-abw_productgroup_wcc/p/aba.abu.abw>
2. Rim joist and first and last joist, applies to deck as well as landing: 2x10 PT

All other joists: 2x8 PT

Stringers: 2x12 PT

Posts: 4x4 PT

1. Spacing between support posts: 81” to 85”
2. 10” sonotube
3. Height of landing: 53”
4. Drawing E
5. QUESTION: you meant to say that inspector must be able to see the connection from inside the house?
6. None planned
7. Drawing E and F
8. The shed underneath the deck? No