461 Cumberland Avenue

* All units will need a hard wired photo electric/battery back-up smoke detector installed in each bedroom.
* All units will need a hard wired photo electric/battery back-up combination smoke/carbon monoxide detector installed in the common area (living room or foyer) of each unit.
* Missing smoke detectors in the common hallways and stairwells will need to be replaced.
* Basement will need to be cleaned of debris and any trash.
* The basement should have a hard wired combination smoke/carbon monoxide detector installed.
* All units should be clearly numbered