Door and Window Schedule for 52 Bolton St

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| # | Name | Width | Height | Material | Notes |
| 1 | American Craftsman | 5’ | 6’8” | Vinyl | Slider |
| 2 |  |  |  |  | Existing Relocated |
| 3 | Hancock Classic | 3’4” | 5’4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51**Egress** |
| 4 | Hancock Classic | 2’ 8” | 4’  | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51 |
| 5 | Hancock Classic | 3’4” | 5’4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51**Egress**  |
| 6 |  | 2’ 8” | 6’ 8” | Wood interior |  |
| 7 |  | 2’ 8” | 6’ 8” | Wood interior |  |
| 8 |  | 2’ 8” | 6’ 8” | Wood interior |  |
| 9 | Not Used |  |  |  |  |
| 10 |  |  |  |  | Existing Exterior |
| 11 |  | 9’ | 8’ |  | Garage Door |
| 12 | Hancock Classic | 2’ 8” | 3’ 4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51 |
| 13 | Hancock Classic | 2’ 8” | 3’ 4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51 |
| 14 | Hancock Classic | 2’ 8” | 3’ 4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51 |
| 15 | Hancock Classic | 2’ 8” | 3’ 4” | White Vinyl | UFactor: 0.26SHG: 0.29VLT: 0.51 |