1150 Brighton Ave Review- 2 hours

1. Take out more pavement at the northern side of the hotel and make the aisle width more conforming to standards.
2. Please submit the following plans:
3. Photometric Plan. The two proposed lighting fixtures, 2 Light Adjustable Option and DCL 570 do not meet standards since not full cutoff and wattage is too high. For LEDs, we ask that they be 3,000 K.
4. Landscaping Plan